# zebra audio

encrypted voice · webrtc · rendezvous · unturf

## call

idle
path: —
input
music mode — raw mic, no echo/noise cancellation (for playing audio through it)

both partners type the same code and hit call. audio is end-to-end encrypted (DTLS-SRTP), peer-to-peer when the network allows, relayed through a TURN server otherwise. the rendezvous server only sees an opaque room id and code-encrypted setup data.

## levels

you
them

## log